  Windows 98 SE

  Introduction:
  -------------
  This document describes the procedure to install Windows 98 SE driver
  for D-Link DGE-528T Gigabit Ethernet Adapter.

  Location of Windows 98 SE Driver : \WIN98SE\DLKRTGB.SYS

  Installing driver for Windows 98 SE:
  ------------------------------------
  Before you start with the installation process, make sure that your
  adapter should be properly installed in your PCI bus slot.
  Executing Windows98 SE, it will auto-detect your system configuration and
  find the adapter hardware.
  (If Windows98 SE does not prompt that it detects the PCI Ethernet Controller,
  there must be something wrong with the DGE-528T Gigabit Ethernet
  adapter or your system enviroment.)

  1. Ask you to select which driver you want to install, select "Search for
  the best driver for your device.(Recommended)".

  2. Insert the DGE-528T Windows driver disk into drive A and specify
  the setup file pathname A:\WIN98SE

  3. Windows98 SE will appear some messages to insert Windows98 SE system disk
  to complete setup step.

  4. Windows98 SE will finish the other installation procedure automatically,
  then Windows98 SE will ask you to restart your system.

