########################################################################
Platform status:
        MODULE: DIR-130
        H/W: A1
        CPU: BCM5836
        switch: BCM5337
        Linux version: linux-router-3.131.35.0(kernel=2.4.20) hnd-tools-3.1.2.3
########################################################################
Released version(SVN): 3492
Released Date: 2009/12/28
F/W Internal Version: 1.23B05
F/W External Version: 1.23
Checksum: 0x582C6E80

Fixed:
	o IPSec support DES IKE
	o URL filter support upto 50 rules.
==========================================================================
Released version(SVN): 3481
Released Date: 2009/12/28
F/W Internal Version: 1.23B04
F/W External Version: 1.23
Checksum:0xE43216A2

Fixed:
	o webfilter can not upload by POST command, eg: upload file from
	hotmail...
	o ipsec site to site with pppoe + ddns can not resolve dns dynamically.

==========================================================================
Released version(SVN): 3474
Released Date: 2009/12/10
F/W Internal Version: 1.23B03
F/W External Version: 1.23
Checksum: 0x1DE62C6A

Fixed:
	o IPSec
	  - support remote site-to-site in full tunnel by
		remote subnet="0.0.0.0/0" from GUI.
	  - support dynamic(from any remote ip) site to site by
		"0.0.0.0" from GUI.
	  - fix l2tp-over-ipsec remote behind NAT-D.
	o GUI
	  - IPSec accept multi local or remote net/mask
		eg: "1.2.3.0/24,1,2.3.4.0/24"

Related Utility:
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_103B03.exe
==========================================================================
Released version(SVN): 3466
Released Date: 2009/11/19
F/W Internal Version: 1.23B02
F/W External Version: 1.23
Checksum: 0xEADB5705

Fixed:
	o IPSec
	  - support remote site-to-site in full tunnel by
		remote subnet="0.0.0.0/0" from GUI.
	  - support dynamic(from any remote ip) site to site by
		"0.0.0.0" from GUI.
	  - fix l2tp-over-ipsec remote behind NAT-D.
	o GUI
	  - IPSec accept multi local or remote net/mask
		eg: "1.2.3.0/24,1,2.3.4.0/24"

Related Utility:
	o VCA Utility: VCAUtility_101B04.exe
	o Java Applet: SSLApplet_101B05.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_103B02.exe
==========================================================================
Released version(SVN): 3426
Released Date: 2009/9/30
F/W Internal Version: 1.23B01
F/W External Version: 1.23
Checksum: 0xC27A1610

Fixed:
	o UI:
	  - After input username and password in login page,
	    cannot press 'Enter' key to login WEBUI (on IE6 and IE7).
	  - In DHCP reservation page, the 26th setting has alignment issue.
	  - No check username be empty in PPPoE/Ru-PPPoE page.
	  - No check WAN physical static IP is valid or not in Ru-PPPoE page.
	  - In Ru-PPPoE page, the maximum MTU is 1492, not 1500.
	  - In DHCP reservation page, the number does not reflect the corrent
	    amount of DHCP reservations remaining. The firewall settings and
	    routing page has the same issue.
	  - Bandwidth control change the input format units and description
	    text from KBytes to Kbits.
	  - VPN Setup Wizard issue:
	    1. Default IPSec Remote Access setting for profile requires NAT-T enabled.
	    2. Default PPTP settings for profile requires MPPE 128-bit.
	    3. align model text from DIR-730 to DIR-130
            4. VPN wizard for pptp, l2tp, ipsec should add annotate for user.
	o PPPoE/Ru-PPPoE, PPTP/Ru-PPTP, and L2TP manual mode still have idle
	  waiting time.
	o Static IP will also shows on client list page. In original D-Link
	  spec, only DHCP IP can displayed on this page.

Related Utility:
	o VCA Utility: VCAUtility_101B03.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_103B01.exe
==========================================================================
Released version(SVN): 3349
Released Date: 2009/7/13
F/W Internal Version: 1.22B12
F/W External Version: 1.22
Checksum: 0xB865D5BE

Fixed:
	o GUI issue
	  A. When incorrect graphical authentication code is entered or
	  incorrect user user credentials are entered, change message to
	  Authentication Failed.
	  B. Login Box is not aligned properly with other boxes.
	  C. Provide examples for the input format so user will understand
	  how to enter an IP range, IP address, multiple IP address that
	  are not in consistent range, or an IP subnet.
	  D. DNS/DDNS is no longer accepted in IPSec site to site Remote
	  IP configuration.
	  E. Align Login Page.

Test:
	o Test max 16384 session.
	  In current RD test max sessions of one Client to one Server 
	  is 3900 sessions(TCP). RD expects max sessions of the DUT is 
	  16384. Please pre-test help to test what max sessions of 
	  the DUT is.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B12.exe
==========================================================================
Released version(SVN): 3338
Released Date: 2009/7/8
F/W Internal Version: 1.22B11
F/W External Version: 1.22
Checksum: 0x765E9267

Fixed:
	o IPSec site to site issue: Remote Local Net/Mask field should
	  not be Router's LAN Net/Mask
	o IPSec site to site issue: Remote Local Net/Mask must different 
	  with Local Net/Mask.
	o Upgrade Utility : Modify the detection and login behavior, and
	  test upgrade from firmware v1.0, 1.10, 1.12, 1.20, 1.21, 1.22.

Test:
	o BT Test with Certificate tools by default. The Default setting
	  is three client and one server. 
	o Schedule rule to follow DIR-655.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B11.exe
==========================================================================
Released version(SVN): 3309
Released Date: 2009/6/30
F/W Internal Version: 1.22B10
F/W External Version: 1.22
Checksum: 0x251CF0A1

Fixed:
	o Bandwidth control page(adv_bandwidth.asp) can accept a network.
	  ex LAN IP: 192.168.0.0, ex Net Mask: 24
	o HTTPS cannot access when remote SSL port be changed to 334 in
	  remote admin page(tools_admin.asp).
	o Schedule issue: (1) add schedule, ex FRI, STA 11:55/pm - 12:5/am,
	  then show wrong day range, and function can't work when apply
	  this schedule.
	o In IPSec settings page, An error shown when remote or local
	  LAN without netmask.
	o UI pop wrong message when (1) add SSLVPN rule without add user
	  group then push 'Save'  -> pop right message, (2) follow step 1
	  then add user group, push 'Save' then cannot save it.

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B10.exe
==========================================================================
Released version(SVN): 3287
Released Date: 2009/6/26
F/W Internal Version: 1.22B09
F/W External Version: 1.22
Checksum: 0x77EC813C

New Feature:
	o IGMP Snopping function closed temporary
	o SSL port cannot be changed by user in SSLVPN page(vpn_ssl.asp),
	  it only can changed in remote ssl settings.
	o Retemo SSL management and SSLVPN can allow multiple IP login.
	  The field of IP address can accept wildcard, single IP address,
	  IP range, and multiple IP using comma or semicolon charactor.
	  Example: 192.168.50.100;172.21.32.0/20,10.0.0.10-10.0.0.20

Fixed:
	o If user connect to remote web but remote web url in web filter
	  deny list or not in allow list, browser will be redirect to
	  reject.html. But reject.html need to authenticate now. It should
	  not be authenticated.

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B09.exe
==========================================================================
Released version(SVN): 3266
Released Date: 2009/6/24
F/W Internal Version: 1.22B08
F/W External Version: 1.22
Checksum: 0x932BC0

New Feature:
	o Schedule rule can support over night or over week.

Fixed:
	o IP range support in web filter cannot work.
	o When router's lan ip is 128.0.0.1 then pptp wan mode fail.
	o In L2TP over IPSec VPN settings page(vpn_pptp.asp).
	  UI always check the Pre-shared Key field even if user
	  choice X.509 certificate option.
	o User can save settings in sslvpn page even if user group is
	  empty.
	o When user save IPSec vpn, he will not set Lan or Remore 
	  Local Net/Mask value. The DUT should check the value.
	o Changed admin password via WIZARD then user can't login anymore.
	o IGMP Snoopying can't be disabled after enabled unless 
	  repower.(dhcp)

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B08.exe
==========================================================================
Released version(SVN): 3229
Released Date: 2009/6/16
F/W Internal Version: 1.22B07
F/W External Version: 1.22
Checksum: 0x51EB1175

Fixed:
	o An error shown on browser when add the 7th SSLVPN rule.
	o IP range support in web filter cannot work.
	  ex: tw.yahoo.com,172.21.1.1 or 172.21.32.1-172.21.32.100
	o Fix D-Track issue HQ20090602000008: DHCP server is not working
	  if there's a client A configured with static IP of 192.168.0.100
	  and another client B configured with dynamic IP. When client B
	  boradcast discovering packet, DIR-130 cannot response anything.
	o Trivial chars attached in SSL remote management title.
	o PPPoE cannot auto reconnect in always-on if PPPoE server send
	  terminating request to PPPoE client or PPPoE server restart.
	o Fix D-Track issue HQ20090611000006: To set over 20 DHCP
	  reservation, DIR-130 will reboot continuously.
	o PPTP/L2TP cannot connect to each other.

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B07.exe
==========================================================================
Released version(SVN): 3201
Released Date: 2009/6/9
F/W Internal Version: 1.22B06
F/W External Version: 1.22
Checksum: 0xC411A43C

New Feature:
	o Graphical authentication disabled in default settings
	o IGMP snooping. User can enable or disable IGMP snooping
	  by UI checkbox(ADVANCED -> Advanced Network).
	o Web URL Filter: User could input IP, Domain, or IP-range.
	  In current, it's support only one rule is IP/Domain or 
	  IP-range in one item.
	  ex:tw.yahoo.com, 123.456.789.100 or 140.135.64.0-140.135.64.255

Fixed:
	o MAC filter issue: LAN can get IP when in block list or not
	  in allow list
	o Click 'Regenerate' button will show an error in login page.
	o SSLVPN fail
	o Enable SSLVPN and disable remote management SSL. User sill
	  can use remote management SSL to login web.
	o Help Description: fix bug for TSD bugs that's #22, #21, #17,
	  #15, #12.
Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B06.exe
==========================================================================
Released version(SVN): 3165
Released Date: 2009/6/1
F/W Internal Version: 1.22B05
F/W External Version: 1.22
Checksum: 0x2A669411

Feature:
	o SSLVPN users are authenticated by HTTPS only, HTTP can't.

Fixed:
	o D-Track issue HQ20090515000007: if set only 'upstream' or
	  'downstream', it will affect another side throughput.
	o PPPoE cannot work
	o Retry: MAC filter deny policy cannot work
	o Retry: Ru-PPTP with MPPE fail
	o Retry: MTU function cannot work in Ru-PPPoE
	o Remote SSL login cannot save log to local

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B05.exe
==========================================================================
Released version(SVN): 3127
Released Date: 2009/5/21
F/W Internal Version: 1.22B04
F/W External Version: 1.22
Checksum: 0xC86B786F

Fixed:
	o IPSec settings cannot specify FQDN including (-) dash charactor
	  in remote address(ex: ipsec-dns.dyndns.org).
	o Network filter deny policy cannot work.
	o DUT cannot connect to PPTP server if PPTP server require MPPE
	  encrypt.
	o DDNS/PPTP/Ru-PPTP server address accept invalid IP address
	  (ex: 192.168.0.456, 255.255.255.0, ...).

Hint:
	o The firmware upgrade utility be able to work if DUT firmware
	  is 1.21 or older version.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B04.exe
==========================================================================
Released version(SVN): 3084
Released Date: 2009/5/14
F/W Internal Version: 1.22B03
F/W External Version: 1.22
Checksum: 0x1190E6C5

Fixed:
	o VPN IPSec site-to-site warning message error. Set VPN IPSec
	  with authentication X.509 certificate. But click save settings
	  button and then appear a warning message about preshared key
	  format(8 - 64 charactors or 16 - 128 hex).
	o When my WAN type is not Ru-PPTP/Ru-PPPoE, it should can't
	  setup WAN_physical on routing settings page.
	o Help description issue: The option name 'Active Session' help
	  description disappear in status help page.
	o Help description issue: The title name 'DDNS' should be the
	  same with option name 'Dynamic DNS'.
	o Help description issue: The button name 'Restore Factory Defaults'
	  should be the same with help pages description 'Restore Device'.
	o Help description issue: The title name 'Automatic time and date
	  configuration' should be the same with 'Automatic time configuration'.
	o Help description issue: The items name 'Admin' and 'DDNS' should
	  be the same with option name 'Admin Setup' and 'Dynamic DNS'.
	o The maximum rule of firewall settings 75 should be the same with
	  help description (50 rules).
	o Remove unnecessary description 'Add', 'Clear', and 'Enable' about
	  DHCP reservations list page.
	o Remove unnecessary description about WAN type 'BigPond'.
	o The server address field for DDNS should avoid user to input
	  illegal IP. For example: '0.0.0.0' or '255.255.255.255'.
	o The 'Server Name/IP' field for PPTP/L2TP and Russia PPTP should
	  avoid user to input illegal IP, for example: '0.0.0.0' or
	  '255.255.255.255'.
	o DUT setup 'Turn MAC Filtering ON and DENY computers listed to
	  access the network' mode on Network Filter page, but this function
	  cannot work.
	o NBNS protocol issue: BUT no check Device Name field on Network
	  Settings page. For example, Input all numerical (12345678), can't
	  open web page by http://12345678 (It will change to IP). Example
	  2, If this field include '"' charactor, the DUT web page can't be
	  opened by IP or Domain Name.
	o In PPPoE settings page. When my service name include '"' charactor,
	  after save settings the service name can't display all string.
	o MTU value function can't work on WAN DHCP, Static, and Ru-PPPoE.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B03.exe
==========================================================================
Released version(SVN): 3071
Released Date: 2009/5/12
F/W Internal Version: 1.22B02
F/W External Version: 1.22
Checksum: 0x9A15E41A

Fixed:
	o admin field show "undefined" wording after upgraded F/W and
	  content can't be modified.
	o after add group account, all accounts can't login.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B02.exe
==========================================================================
Released version(SVN): 2991
Released Date: 2009/4/30
F/W Internal Version: 1.22B01
F/W External Version: 1.22
Checksum: 0x7535C6E3

Feature:
	o Graphical Authentication (user group cannot working temporary)
	o The maximum NAT concurrent session extends to 16384

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_102B01.exe
==========================================================================
Released version(SVN): 3057
Released Date: 2009/5/8
F/W Internal Version: 1.21B19
F/W External Version: 1.21
Checksum: 0x31EEDEC0

Fixed:
	o Fix D-Track issue: VPN rules can be set more than 25 profiles.
	  But as the WEB UI display, we only support 25 profiles.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_101B19.exe
==========================================================================
Released version(SVN): 2911
Released Date: 2009/4/20
F/W Internal Version: 1.21B18
F/W External Version: 1.21
Checksum: 0xDF29280B

Fixed:
        o Fix D-Track issue: In PPPoE WAN mode, DUT don't response PADR
	  (and goto next stage). Since our PADI packet including empty
	  service name field. But PPPoE server reply PADO packet had their
	  service name.
	o Fix D-Track issue: In russia-PPTP, the IGMP packet had source IP
	  is DIR-130/330 tunnel IP. The source IP of IGMP packet should be
	  WAN physical IP.

Related Utility:
        o VCA Utility: VCAUtility_101B02.exe
        o Java Applet: SSLApplet_101B04.jar
        o Firmware upgrade utility: DIR130_FirmwareUpgrade_101B18.exe
==========================================================================
Released version(SVN): 2896
Released Date: 2009/4/16
F/W Internal Version: 1.21B17
F/W External Version: 1.21
Checksum: 0x93E299A7

Fixed:
	o Fix D-Track issue: remote PC can't access to DIR-130/330 LAN site
	  after the PPTP tunnel established and wait more than 15 minutes.
	  The remote PC and DUT WAN both are PPPoE mode.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
	o Firmware upgrade utility: DIR130_FirmwareUpgrade_101B17.exe
==========================================================================
Released version(SVN): 2877
Released Date: 2009/4/13
F/W Internal Version: 1.21B16
F/W External Version: 1.21
Checksum: 0x3A6F59A8

Fixed:
	o Fix D-Track issue: In PPPoE WAN mode, DUT only send out two
	  times PADI packets after device power-on. If ATU-R power-on
	  after DUT send out two times PADI, PPPoE cannot connect.
	o Fix D-Track issue: In PPTP/Ru-PPTP WAN mode, DUT cannot send
	  Call-Disconnect-Notify packet before reboot.
	o Fix D-Track issue: The upload bandwidth is not functioning for
	  PPPoE/PPTP/L2TP.
	o Fix D-Track issue: In PPPoE WAN mode, DUT don't response PADR
	  (and goto next stage). Since our PADI packet including empty
	  service name field. But PPPoE server reply PADO packet had their
	  service name.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B04.jar
==========================================================================
Released version(SVN): 2861
Released Date: 2009/3/30
F/W Internal Version: 1.21B15
F/W External Version: 1.21
Checksum: 0x519760FD

Fixed:
        o Fix D-Track issue: Ru-PPTP cannot auto reconnect if user plug-out
          the PPTP server physical link over 200 seconds.

Related Utility:
        o VCA Utility: VCAUtility_101B02.exe
        o Java Applet: SSLApplet_101B04.jar
==========================================================================
Released version(SVN): 2836
Released Date: 2009/3/4
F/W Internal Version: 1.21B14
F/W External Version: 1.21
Checksum: 0x6B5C2C97

Fixed:
	o Fix D-Track issue: L2TP tunnel establish fail with tp.corbina.ru
	o Fix D-Track issue: PPTP/Ru-PPTP cannot auto reconnect

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B02.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B14.exe
==========================================================================
Released version(SVN): 2827
Released Date: 2009/3/2
F/W Internal Version: 1.21B13
F/W External Version: 1.21
Checksum: 0x9D4B118

Fixed:
	o Cannot connect to tp.corbina.ru use domain name.
	o Stable VCA utility version is 1.01BXX, not 1.02BXX.

Related Utility:
	o VCA Utility: VCAUtility_101B02.exe
	o Java Applet: SSLApplet_101B02.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B13.exe
==========================================================================
Released version(SVN): 2820
Released Date: 2009/3/2
F/W Internal Version: 1.21B12
F/W External Version: 1.21
Checksum: 0xB93A57FD

Fixed:
	o D-Track bug: cannot connect to tp.corbina.ru using L2TP client.
	o Stable VCA utility version is 1.01BXX, not 1.02BXX.

Related Utility:
	o VCA Utility: VCAUtility_101B01.exe
	o Java Applet: SSLApplet_101B02.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B12.exe
==========================================================================
Released version(SVN): 2814
Released Date: 2009/2/18
F/W Internal Version: 1.21B11
F/W External Version: 1.21
Checksum: 0x6CE20AA6

Fixed:
        o delete all sslvpn rules, https remote cannot login

Related Utility:
        o VCA Utility: VCAUtility_102B01.exe
        o Java Applet: SSLApplet_100B23.jar
        o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B11.exe
==========================================================================
Released version(SVN): 2810
Released Date: 2009/2/17
F/W Internal Version: 1.21B10
F/W External Version: 1.21
Checksum: 0xA8BF8640

Fixed:
        o if https remote disabled, SSLVPN user cannot login to auth.asp

Related Utility:
        o VCA Utility: VCAUtility_102B01.exe
        o Java Applet: SSLApplet_100B23.jar
        o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B10.exe
==========================================================================
Released version(SVN): 2794
Released Date: 2009/2/9
F/W Internal Version: 1.21B09
F/W External Version: 1.21
Checksum: 0xE109F250

Fixed:
        o if DMZ enabled, SSLVPN cannot work
	o In the network setting page (lan.asp) DHCP reservations list,
	  IP address field width so short that the field be cuted.
	o In routing status page (st_route.asp), web frame is too wider
	  after add rules.
	o Enter routing status page is too slow.

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B22.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B09.exe
==========================================================================
Released version(SVN): 2787
Released Date: 2009/2/5
F/W Internal Version: 1.21B08
F/W External Version: 1.21
Checksum: 0x1E82BE07

Fixed:
        o Enable DMZ, but https remote and SSL VPN cannot work.
	o Page st_route.asp cannot display any static routing information.
	o "Computer Name" does not be displayed automatically after the DUT
	  has been had some configures.
	o In the network setting page (lan.asp) DHCP reservations list,
	  IP address field width so short that the field be cuted.
	o DHCP client Release/Renew behavior modified.
	  step1. goto page st_device.asp.
	  step2. click 'DHCP Release', page reload and IP/mask/gw information be 0.0.0.0
	  step3. click 'DHCP Renew', page reload and Release/Renew button both are disabled.
	  step4. wait 15 seconds, the page will auto reload. Now, Release/Renew button both
	         are enabled and IP information displayed on UI.

Related Utility:
        o VCA Utility: VCAUtility_100B12.exe
        o Java Applet: SSLApplet_100B22.jar
        o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B08.exe
==========================================================================
Released version(SVN): 2776
Released Date: 2009/1/23
F/W Internal Version: 1.21B07
F/W External Version: 1.21
Checksum: 0xFECCE9C0

Fixed:
	o hide the ssl only checkbox in vpnssl page (vpn_ssl.asp).

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B22.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B07.exe
==========================================================================
Released version(SVN): 2772
Released Date: 2009/1/22
F/W Internal Version: 1.21B06
F/W External Version: 1.21
Checksum: 0x2A79D9E5

Fixed:
	o add SMTP server port field into log setting page
	o hidden page changed according to D-Link spec.

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B22.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B06.exe
==========================================================================

Released version(SVN): 2750
Released Date: 2009/1/7
F/W Internal Version: 1.21B05
F/W External Version: 1.21
Checksum: 0xC24BDC18

Fixed:
	o Fix D-Track issue HQ20091124000007, unable to establish L2TP
	  over IPSec VPN client connections from MAC OS v10.4.11.
	o PSK always check validation regardless VPN type is L2TP or
	  L2TP over IPSec.

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B22.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B05.exe
==========================================================================
Released version(SVN): 2741
Released Date: 2008/12/16
F/W Internal Version: 1.21B04
F/W External Version: 1.21
Checksum: 0x9528F2B8

Fixed:
	o oray DDNS cannot working

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B21.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B04.exe
==========================================================================
Released version(SVN): 2715
Released Date: 2008/12/08
F/W Internal Version: 1.21B03
F/W External Version: 1.21
Checksum: 0x27D64A7F

Feature:
	o SSL port options: user can modify https login port in tools_admin.asp
	  and ssl_vpn.asp (default is 443 port).
	o SSL Only options: if SSL Only is checked, sslvpn tunnel only working
	  at SSL mode. The VCA also ignore IPSec negotiation and starting at
	  SSL negotiation.
	o add oray DDNS option in tools_ddns.asp

Fixed:
	o IPSec pre-shared key length must be 8-64 charactors or 16-128 hex.
	o IPSec remote user sometimes fail in russia pptp (buffer not clear).
	o L2TP over IPSec remote user sometimes fail (empty dns field).
	o DDNS cannot working

Related Utility:
	o VCA Utility: VCAUtility_100B11.exe
	o Java Applet: SSLApplet_100B21.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B03.exe
==========================================================================
Released version(SVN): 2683
Released Date: 2008/11/27
F/W Internal Version: 1.21B02
F/W External Version: 1.21
Checksum: 0x2DCAFE98

Feature:
	o VPN IPSec pre-shared key length must be 8 - 64 charactors.

Fixed:
	o Fix D-Track issue HQ20081111000002-DIR-330_DIR-330 Routing issue on
	  manual mode and dial-on demand mode.

Related Utility:
	o VCA Utility: VCAUtility_100B11.exe
	o Java Applet: SSLApplet_100B20.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B02.exe
==========================================================================
Released version(SVN): 2675
Released Date: 2008/11/20
F/W Internal Version: 1.21B01
F/W External Version: 1.21
Checksum: 0x817AAB6B

Fixed:
	o Fix D-Track issue HQ20080903000004 firewall issue:
	  Here are two firewall rules, one allow and one deny, allow first
	  and deny secondly:

	  1. Allow one IP of LAN to WAN, all protocol, ex: 192.168.0.100
	  2. Deny all IP of LAN to WAN, all protocol.

	  The IP 192.168.0.100 still denied by router, but we want the
	  firewall rules sequence according to UI shows. So, The IP
	  192.168.0.100 should be allowed.
	o Fix D-Track issue HQ20081111000002-DIR-330_DIR-330 Routing issue.
	  The WAN type is russia pptp + static ip, router cannot find pptp
	  server if pptp server IP is different network with WAN IP.

Related Utility:
	o VCA Utility: VCAUtility_100B11.exe
	o Java Applet: SSLApplet_100B19.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_101B01.exe
==========================================================================
Released version(SVN): 2729
Released Date: 2008/12/12
F/W Internal Version: 1.20B39
F/W External Version: 1.20
Checksum: 0xC3129223

Fixed:

	o DMZ fail if port forwarding enable
	o Bandwidth control page lose header description

Related Utility:
	o VCA Utility: VCAUtility_100B12.exe
	o Java Applet: SSLApplet_100B20.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B18.exe
==========================================================================
Released version(SVN): 2668
Released Date: 2008/11/19
F/W Internal Version: 1.20B38
F/W External Version: 1.20
Checksum: 0xC7BB910C

Fixed:
	o denying page still has authentication.
	o redirect page fail in remote_decision.asp

Related Utility:
        o VCA Utility: VCAUtility_100B11.exe
        o Java Applet: SSLApplet_100B19.jar
        o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B17.exe
==========================================================================
Released version(SVN): 2660
Released Date: 2008/11/18
F/W Internal Version: 1.20B37
F/W External Version: 1.20
Checksum: 0x739A3BCE

Fixed:
	o URL filter bugs: deny page need username/password

Related Utility:
	o VCA Utility: VCAUtility_100B11.exe
	o Java Applet: SSLApplet_100B19.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B16.exe
==========================================================================
Released version(SVN): 2617
Released Date: 2008/10/21
F/W Internal Version: 1.20B36
F/W External Version: 1.20
Checksum: 0x5E887C28

Fixed:
	o remove wireless related description or key words in following webpages:
	  - tools_admin.asp
	  - st_log_settings.asp
	  - adv_bandwidth.asp
	  - support_tools.asp
	  - support_adv.asp
	  - support_men.asp
	  - support_internet.asp
	  - remote_dicision.asp
	  - vpn_ssl.asp

Related Utility:
        o VCA Utility: VCAUtility_100B10.exe
        o Java Applet: SSLApplet_100B17.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B15.exe
==========================================================================
Released version(SVN): 2605
Released Date: 2008/10/20
F/W Internal Version: 1.20B35
F/W External Version: 1.20
Checksum: 0x6E385E6C

Fixed:
	o remove wireless related description from index.asp, vpn_ssl.asp,
	  and adv_bandwidth.asp

Related Utility:
	o VCA Utility: VCAUtility_100B10.exe
	o Java Applet: SSLApplet_100B17.jar
==========================================================================
Released version(SVN): 2591
Released Date: 2008/10/14
F/W Internal Version: 1.20B34
F/W External Version: 1.20
Checksum: 0x6D6D41F0

Fixed:
	o cannot connect to the remote pptp server (different network with
	  WAN physical).
	o in pptp/rupptp, pppoe/rupppoe, l2tp pages, if AlwaysOn or Manual
	  checked, the idle time should be disable.

Related Utility:
	o VCA Utility: VCAUtility_100B06.exe
	o Java Applet: SSLApplet_100B15.jar
==========================================================================
Released version(SVN): 2581
Released Date: 2008/10/9
F/W Internal Version: 1.20B33
F/W External Version: 1.20
Checksum: 0x92B55C4D

Fixed:
	o In russia pptp mode, PC cannot establish tunnel to WAN physical
	  IP which PC is the same network with WAN physical IP.

Related Utility:
	o VCA Utility: VCAUtility_100B06.exe
	o Java Applet: SSLApplet_100B15.jar
==========================================================================
Released version(SVN): 2579
Released Date: 2008/10/9
F/W Internal Version: 1.20B32
F/W External Version: 1.20
Checksum: 0x459AD3F2

Fixed:
	o In russia pptp page(wan_rupptp.asp), if Always-On is selected,
	  Idle time field should be disabled, otherwise is enabled.
	o In russia pptp mode, PC cannot establish tunnel to WAN physical
	  IP which PC is the same network with WAN physical IP.
	o In russia pptp page(wan_rupptp.asp), Server IP/Name field extends
	  to 64 charactors.

Related Utility:
	o VCA Utility: VCAUtility_100B06.exe
	o Java Applet: SSLApplet_100B15.jar
==========================================================================
Released version(SVN): 2560
Released Date: 2008/10/2
F/W Internal Version: 1.20B31
F/W External Version: 1.20
Checksum: 0xC0BACC73

Fixed:
	o in russia mode, rc always restart at 30 seconds interval time,
	  because WAN dhcpc get a new IP which lease time is 60 seconds.
	o if dhcpc dns(WAN gets) is not in the same network with WAN IP,
	  these dns IPs add in routing table.
	o allow russia-pptp server name be a FQDN or IP address.
	o extends russia-pptp server name field to 64 charactors.

Related Utility:
	o VCA Utility: VCAUtility_100B05.exe
	o Java Applet: SSLApplet_100B14.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B14.exe
==========================================================================
Released version(SVN): 2537
Released Date: 2008/9/23
F/W Internal Version: 1.20B30
F/W External Version: 1.20
Checksum: 0x34DDD559

Fixed:
	o IPSec site to site tunnel establishing fail, when pppoe or
	  pptp disconnect in russia mode.
	o If two routers both use pppoe or pptp to establishing site to
	  site tunnel, tunnel was fail. ex: pptp(pppoe) <-> pptp(pppoe)

Related Utility:
	o VCA Utility: VCAUtility_100B05.exe
	o Java Applet: SSLApplet_100B14.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B13.exe
==========================================================================
Released version(SVN): 2522
Released Date: 2008/9/12
F/W Internal Version: 1.20B29
F/W External Version: 1.20
Checksum: 0x93283F76

Fixed:
        o In dual access mode, ipsec site to site tunnel establishing fail.
        o After change LAN ip, wireless client still get old ip.

Related Utility:
        o VCA Utility: VCAUtility_100B04.exe
        o Java Applet: SSLApplet_100B14.jar
==========================================================================
Released version(SVN): 2501
Released Date: 2008/9/3
F/W Internal Version: 1.20B28
F/W External Version: 1.20
Checksum: 0xA441DE4A

Feature:
        o In ssl applet page, if OS and browser both equal to 'Vista' and
          'Firefox' simultaneously, then ssl applet page will denied running
          and pop-up warning message.

Related Utility:
        o VCA Utility: VCAUtility_100B04.exe
        o Java Applet: SSLApplet_100B14.jar
==========================================================================
Released version(SVN): 2484
Released Date: 2008/8/25
F/W Internal Version: 1.20B27
F/W External Version: 1.20
Checksum: 0xB9884A99

Feature:
	o drop SSDP form wan in russia mode

Related Utility:
        o VCA Utility: VCAUtility_100B03.exe
        o Java Applet: SSLApplet_100B13.jar
==========================================================================
Released version(SVN): 2469
Released Date: 2008/8/20
F/W Internal Version: 1.20B26
F/W External Version: 1.20
Checksum: 0x7A142BD0

Feature:
	o The welcome message displayed on http/https login dialog.
	  ex: "Welcome to the [device_name]".
	o Device name can set in lan.asp
	o User connect to the router can using the following URL:
	  http://[device_name].

Related Utility:
        o VCA Utility: VCAUtility_100B03.exe
        o Java Applet: SSLApplet_100B13.jar
==========================================================================
Released version(SVN): 2438
Released Date: 2008/8/8
F/W Internal Version: 1.20B25
F/W External Version: 1.20
Checksum: 0xA6864CCF

Fixed:
	o utility URL error in checklist(chklst.txt/version.txt).

Related Utility:
        o VCA Utility: VCAUtility_100B02.exe
        o Java Applet: SSLApplet_100B11.jar
==========================================================================
Released version(SVN): 2427
Released Date: 2008/8/7
F/W Internal Version: 1.20B24
F/W External Version: 1.20
Checksum: 0x856F8DCF

Feature:
        o If openvpn tunnel disconnect under abnormal situation, VCA utility
          will connection retry 45 seconds. When 45 seconds passed, VCA utility
          will terminate (fred).

Related Utility:
        o VCA Utility: VCAUtility_100B01.exe
        o Java Applet: SSLApplet_100B10.jar
==========================================================================
Released version(SVN): 2408
Released Date: 2008/7/18
F/W Internal Version: 1.20B23
F/W External Version: 1.20
Checksum: 0xDCE544D0

Fixed:
        o The host ping LAN IP from WAN, the LAN host also has response(peter).

Related Utility:
        o VPN Utility: DIR130_VPNUtility_100B03.exe
        o SSL Utility: DIR130_SSLUtility_100B09.exe
        o Java Applet: SSLApplet_100B09.jar
==========================================================================
Released version(SVN): 2370
Released Date: 2008/6/12
F/W Internal Version: 1.20B22
F/W External Version: 1.20
Checksum: 0xDE90B04D

Feature:
        o User can select how to install ssl utility by ssl java applet.
          Download from one of area or install from specify 'setup.exe' file(Fred).

Related Utility:
        o VPN Utility: DIR130_VPNUtility_100B03.exe
        o SSL Utility: DIR130_SSLUtility_100B09.exe
        o Java Applet: SSLApplet_100B08.jar
	o Firmware Upgrade Utility: DIR130_FirmwareUpgrade_100B09.exe
==========================================================================
Released version(SVN): 
Released Date: 2008/6/11
F/W Internal Version: 1.20B21
F/W External Version: 1.20
Checksum: 0x84A64D98

Feature:

Fixed:
Feature:
	o DHCP client list from GUI will detect alive of client host. (peter)
	o Firmware upgrade need not to restore default. So far,
	    Those known functions in this issue are:
		o PPTP, L2TP server auth with group.	(geoffrey)
		o IPSec format from v1.00 to v1.20.	(peter)
		o Admin password.			(fred)
	o Port Forwarding should be applied to not only from WAN to WAN,
       	also LAN to WAN.
	o user can select how to down ssl utility by ssl java applet
Fixed:
	o telnet with empty password(default should be "cameo"), (peter).
	o VLC media stream by different subnet from WAN.(peter)
	o set none to default for pptpd mppe (geoffrey)
	o IPSec L2TP can not work - service does not activiate (fred)
	o VPN server (pptp/l2tpoipsec) and IPsec fail (geoffrey  fred)
	o delete l2tp over ipsec rule will disable L2TP rule (geoffrey)
	o When L2TP is enabled and work, if we delete the other disabled rules,
       	the L2TP will can't work. (KenWu)
	o L2TP works only when a 'l2tp over ipsec' rule on router,
	  and remote user will get wrong IP range. (Fred)
	o After device reboot, DHCPD can not keep records of clients list
       	status. (peter)
	o DHCPC LAN client PC switch to static IP, DHCP client list can not 
	update. (peter)
	o Russia-PPTP and Russia-PPPoE   DHCP segment cannot be accessed after
       	PPP link up (geoffrey)
	o Remote admin "page not found" access error from WAN.


Confirm:
	o Over all traffic to IPSec tunnel, including DNS service.
	o If original firmware version is 1.00, router can't auto reboot after
       	firmware upgrade to newly version by utility. So, F/W upgrade utility
       	display hint message about reboot after upgrade successful by user
       	itself.
	o 'l2tp' rule and 'l2tp over ipsec' rule are both exist. After delete
       	'l2tp over ipsec' rule, Client PC enable to connect to the router using
       	l2tp tunnel, and the l2tp client must get correct IP range from 'l2tp'
       	rule.

Related Utility:
	o VPN Utility: DIR130_VPNUtility_100B03.exe
	o SSL Utility: DIR130_SSLUtility_100B09.exe
	o Java Applet: SSLApplet_100B08.jar
==========================================================================
Released version(SVN): 
Released Date: 2008/5/15
F/W Internal Version: 1.20B20
F/W External Version: 1.20
Checksum: 

Feature:

Fixed:
o in auth.asp, 'Stop installation' and normal status message exchange with
  each other at first install utility.
o in ipsec page (vpn_ipsec.asp) and l2tp over ipsec page (vpn_pptp.asp).
  if udp:500 or any:500 is used in port forwarding, these pages will pop-up
  warning message.
o udhcpd can not display hostname of dhcp client.
==========================================================================
Released version(SVN): 2243
Released Date: 2008/5/5
F/W Internal Version: 1.20B19
F/W External Version: 1.20
Checksum: 0x5FB1E506

Feature:
o adjust applet width and height in cgi 'file_exist'.
o modify applet status message in auth.asp, according to d-link request.
o modify auth.asp to disable scroll bar displayed on browsers.

Fixed:
o avoid 'l2tp overipsec' connection without establishing ipsec tunnel.
o avoid password blank in usergroup page.
o dhcp renew fail in russia pppoe.
o when in PPPoE, should pop-up message between 200 - 1500.
o when in PPTP and L2TP, should pop-up message between 200 - 1400.
==========================================================================
Released version(SVN): 2198
Released Date: 2008/4/18
F/W Internal Version: 1.20B17
F/W External Version: 1.20
Checksum: 0x27094127

Feature:
o add the description about account accessible on ADMINISTRATOR SETTINGS.
o restore to default settings when first reboot after firmware upgrade
  success, regardless which firmware version from.
o if account in sslvpn group and not in remote admin group, page will
  redir to remote admin page. if account in remote admin group and not
  in sslvpn group, page will redir to ssl page. if account both in
  remote admin group and sslvpn group, page will redir to remote admin
  page.
o sslvpn account cannot access remote admin page, and remote admin
  account cannot access sslvpn page.

Fixed:
o in VPN-IPSEC page, group account can't remove from rule when account
  has in SSL of remote manage.
o remove the User Login Name and User Password description in ACMIN of HELP.
o Modify help hints for bandwidth control format is different with others.
==========================================================================
Released version(SVN): 2176
Released Date: 2008/4/16
F/W Internal Version: 1.20B16
F/W External Version: 1.20
Checksum: 0xB97FD563

Feature:
o if account both in remote manager group and sslvpn group, redirect to
  the ssl page.

Fixed:
o when user add another group, the original account will disappear.
o router crash when save settings in tools_admin.asp page. When a) add
  a group to right side, b) add 2 group with 'ctrl', the save.
o in admin setup page, right side account dispear when push '<<' directly.
o in admin setup page, right side account no 'ctrl' or 'shift' function.
o in admin setup page, pop wrong message after delete ('>>') top account
  from right side.
o in VPN-IPSEC page, WEB pop wrong when user try to add IPSEC rule.
o router crash when use virtual server/ftp.
o CA is empty, so user can't save without enable ssl remote manager.
==========================================================================
Released version(SVN): 2143
Released Date: 2008/4/10
F/W Internal Version: 1.20B15
F/W External Version: 1.20
Checksum: 0x375C19FB

Feature:
o add del function for user group in vpn_ssl.asp and tools_admin.asp

Fixed:
o in 'check now' function, firmware check miss maybe occur, because of
  string comparing problem.
o if disable remote ssl login or ssl vpn login, https will not terminate.
==========================================================================
Released version 120B14
Released Date: 2008/4/3
MODULE: DIR-130
F/W: 1.20B14
H/W: A1

Feature:
o add multi-group selection in remote admin and VPN settings page.
o add ESMTP support in log settings page.
o https support for remote admin.
o remote account can login into remote admin page, and ssl account can
  login into ssl page (auth.asp).
o create a newly check list file, called 'version.txt'.

Fixed:
o In auth.asp page. If applet jar url is incorrect or jar file not exist
  in wrpd.dlink.com.tw specific folder, auth.asp page will show error
  messages.
o Adjust firmware check now page. After click 'check now' button, newest
  firmware information will display at another table on page.
o deny all of non-Windows operating system login into ssl page.

==========================================================================
Released version 120B11
Released Date: 2008/3/5
MODULE: DIR-130
F/W: 1.20B11
H/W: A1

Feature:
o add tftpd for firmware upgrade
o remove bigpond from UI
o add firmware update utility

==========================================================================
Released version 120B10
Released Date: 2008/2/22
MODULE: DIR-130
F/W: 1.20B10
H/W: A1

Fixed:
o Fix vpn firewall parse token problem
o DIR-130 and DIR-330 use different utility from this firmware

==========================================================================
Released version 120B9
Released Date: 2008/2/4
MODULE: DIR-130
F/W: 1.12B9
H/W: A1

Fixed:
o Fix the HTML about download JVM

==========================================================================
Released version 120B8
Released Date: 2008/2/1
MODULE: DIR-130
F/W: 1.12B8
H/W: A1

Fixed:
o Fix the HTML about download JVM
o Update the URL about query SSLApplet_100.jar and SSLUtility_100.exe

==========================================================================
Released version 120B7
Released Date: 2008/1/31
MODULE: DIR-130
F/W: 1.12B7
H/W: A1

Fixed:
o Let ssl vpn utility workable on firefox

==========================================================================
Released version 120B6
Released Date: 2008/1/29
MODULE: DIR-130
F/W: 1.12B6
H/W: A1

Fixed:
o Let ssl vpn utility workable on firefox

==========================================================================
Released version 120B5
Released Date: 2008/1/16
MODULE: DIR-130
F/W: 1.12B5
H/W: A1

Fixed:
o Auto dowanlod ActiveX from wrpd

Feature:
o 802.1q and 802.1p

==========================================================================
Released version R2157
Released Date: 2007/08/08
MODULE: DIR-130
F/W: 1.10
H/W: A1

FIX TSD bugs
o Fixed a invalid config file be restored: return a failure message
o Pop confirm message which "Restore factory default" and "Reboot device"
	and "Firmware upgrade"
o Fixed UI messages stream buffer size of responsed ping: "ali" to "alive"
o Fixed blank of DATE TIME MANUAL.
o UPnP display of "Model Number": "DIR-130/330" as "DIR-130", and Description.
o WPS text description
o Firewall block LAN to LAN, WAN to WAN.
o STATUS->VPN type: "l2tpd" to "L2TP", "pptpd" to "PPTP"
o VPN select list of UserGroup(s) will list not-empty only.
o "Daylight saving" activity only while NTP enabled.
o DHCPD server still reserves older records when LAN IP is modified.
o LOG page enable with NTP, DDNS enable will pending system.

==========================================================================
Released version R2155
Released Date: 2007/07/31
MODULE: DIR-130
F/W: 1.10
H/W: A1

Fixed
o L2TP could not save to NVRAM from UI.
o IPSec, L2TP UI

Issues
o Log page with NTP enable will failure(block by awk...)

==========================================================================

Released version R2153
Released Date: 2007/07/30
MODULE: DIR-130
F/W: 1.10
H/W: A1


For Pretest TSD
Main features of DIR-130

Updated:

Fixed bugs
o X509 size limitation 2048 bytes.
o X509 deleted protection while profile inused by IPSec profile.
o Resize connection session up to 8192
o Profile name of IPSec, prot forwarding, application, mac filter, url,
	firewall, certificate, and user group pages, which should not apply
	when name field are existed already previously.
o DHCP reservation should be limited by DHCP server assgined ranges.


==============================================================================

Released version v2151
MODULE: DIR-130
F/W: 1.10
H/W: A1


For Pretest TSD
Main features of DIR-130

Updated:

o DDNS UI status.
o Certificates validity check.
o Save log file.
o UPNP bug fixed.
o Virtual server UI bug.
o Fixed bug: Update firmware from 1.00 to 1.10 GUI login & password become to blank.
o Application server protocol tcp & udp bug.

Fixed bugs:
 3689 vpn__1. X.509 + Aggressive mode „³Link FAIL 2. XAUTH + X.509 +MAIN mode „³ Link FAIL 3. XAUTH + PSK + Aggressive mode „³ Link FAIL 4. CAST /MOD5„³Link FAIL 5.. IKE LIFE < 1500 , > 77777„³Link FAIL 
--------------------------------------------------------------------------------
 
 3690 vpn__VPN link is not stable when NAT-T enable 
--------------------------------------------------------------------------------
 
 3691 vpn__Router crash when assign different CA to different vpn rules. 
--------------------------------------------------------------------------------
 
 3692 vpn__IPSEC and l2tp-ipsec can¡¦t coexist 
--------------------------------------------------------------------------------
 
 3693 Port forwarding __1. Port forwarding fail when add a port range (only single port is ok) 2. Port 0 should be prohibited 
--------------------------------------------------------------------------------
 
 3694 Application rule__Application rule fail when user sets rule by manual not from list 
--------------------------------------------------------------------------------
 
 3695 Web filter__Web filter¡¥s frame becomes wider when enter this page. 
--------------------------------------------------------------------------------
 
 3696 Routing__Routing function fail  
