  Windows ME

  Introduction:
  -------------
  This document describes the procedure to install Windows ME driver
  for D-Link DGE-528T Gigabit Ethernet Adapter.

  Location of Windows ME Driver : \WINME\DLKRTGB.SYS

  Installing driver for Windows ME:
  ---------------------------------
  Before you start with the installation process, make sure that your
  adapter should be properly installed in your PCI bus slot.
  Executing Windows ME, it will auto-detect your system configuration and
  find the adapter hardware.
  (If Windows ME does not prompt that it detects the PCI Ethernet Controller,
  there must be something wrong with the DGE-528T Gigabit Ethernet
  adapter or your system enviroment.)

  1. Ask you to select which driver you want to install, select "Specify the
  location of the driver(Advanced)".

  2. Insert the DGE-528T Windows driver disk into drive A and specify
  the setup file pathname A:\WINME

  3. Windows ME will appear some messages to insert Windows ME system disk
  to complete setup step.

  4. Windows ME will finish the other installation procedure automatically,
  then Windows ME will ask you to restart your system.

