  Windows XP 64-Bit

  Introduction:
  -------------
  This document describes the procedure to install Windows XP 64-Bit driver
  for D-Link DGE-528T Gigabit Ethernet Adapter.

  Location of Windows XP 64-Bit Driver : \WINXP64\DLKRT64.SYS

  Installing driver for Windows XP 64-Bit:
  ----------------------------------------
  Before you start with the installation process, make sure that your
  adapter should be properly installed in your PCI bus slot.
  Executing Windows XP 64-Bit, it will auto-detect your system configuration
  and find the adapter hardware.
  (If Windows XP 64-Bit doesn't prompt that it detects the Ethernet Controller,
  there must be something wrong with the DGE-528T Gigabit Ethernet
  adapter or your system environment.)

  1. The WinXP64 builds-in the driver. If you want to update new driver,
  please choose "Don't search, I will choose the driver to install" of
  "Install from a list or specific location [Advanced]".

  2. Insert the DGE-528T Windows driver disk into drive A and specify
  the setup file pathname A:\WINXP64

  3. The Windows XP 64-Bit will start to copy the drivers into the system.

  4. Windows XP 64-Bit will finish the other installation procedure
  automatically.

