**Installation Introductions of DWM-15X series in Ubuntu System**

The installation steps of DWM-156 in Ubuntu system are as follows.

1. **Plug the dongle with SIM card (disable the PIN code first) into the USB port of your computer.**

**1.1 Check the device with command:**

ls /dev/sr\*

【Return】



If the system returns as follows, it means the software has been installed before.

![C:\Users\lijinrong\AppData\Roaming\Tencent\Users\962275147\QQ\WinTemp\RichOle\AJ5~]%${O0J5ZZV5O`8J4L5.jpg]()

Uninstall it with command:

sudo dpkg –r 3g-modem-connection-dtlwg-d310a-i386

[**Notice**: the red one means the name of the software that has been installed.]

**1.2 Mount.**

Use command:

sudo mount /dev/sr0  /mnt

【Return】



**1.3 Check the result of mount, using command:**

cd /mnt

 ls

【Return】



If the system returns as above, then succeed.

1. **Installation**

Install the software with command:

sudo dpkg -i 3g\_modem\_connect\_DTLWG\_D310\_i386.deb

[**Notice**: use 3g\_modem\_connect\_DTLWG\_D310\_i386.deb in 32-bit system and 3g\_modem\_connect\_DTLWG\_D310\_amd64.deb in 64-bit system]

【Return】



The installations are finished when system prompts “Install finished”.

**3. Connect to the Internet**

1. **Dial up**

After you finished the installation, please replug the dongle, it will dial up automatically. The dial operation may continue for three minutes, please wait…

1. **Check the network is connected**

You could open your browser, and view the webpage to check.